	METERING PUMP DATA SHEET
1	PROJECT			JOB NO.
2	PURCHASER			ITEM NO.
3	SERVICE			QUANTITY
4	OPERATING CONDITIONS			PERFORMANCE
5	LIQUID			PUMP MODEL		KPV-161L-SF-S
6	PUMPING TEMP (℃)			PUMPING TEMP (℃)		0~100℃
7	AMBIENT TEMP (℃)			VISCOSITY (cP)		MAX 1000
8	SPECIFIC GRAVITY			CAPACITY (mL/min)		MAX 100
9	VISCOSITY (cP)			DISCHARGE PRESS (bar)		MAX 160
10	CAPACITY (mL/min)			STROKE SPEED (SPM)		58
11	DISCHARGE PRESS (bar)			STROKE LENGTH (㎜)		10
12	SUCTION PRESS (bar)			PLUNGER DIA (㎜)		16
13	NPSH AVAILABLE (m)			NPSH REQUIRED (m)		3
14	LOCATION			BHP RATED (kW)		0.118
15	CONSTRUCTION			MATERIALS
16	PUMP TYPE		PLUNGER	HEAD		STS316
17	FEED NUMBER		SINGLE	PLUNGER		STS316+CQ
18	VALVE TYPE		CHECK BALL	CHECK BALL		STS316
19	VALVE NUMBER		DOUBLE	BALL GUIDE		STS316
20	CONNECTION TYPE		FLANGE	BALL SEAT		STS316
21	SUCTION SIZE		KS 20K 15A RF	GLAND PACKING		PTFE+ARAMID
22	DISCHARGE SIZE		KS 63K 15A RF	VALVE GASKET		PTFE+PFA
23	CONTROL			DRIVE (MOTOR)
24	TYPE		MANUAL	TYPE		TEFC
25	METHOD		STROKE ADJUSTMENT	MANUFACTURER		SHINKANG
26	ADJUSTMENT RANGE		10~100%	OUTPUT (kW)		0.2
27	PAINTING COLOR			VOLTAGE/PHASE/HERTZ		220/380V / 3Ø / 60Hz
28	PUMP (Munsell No)		0.6PB 4.8/10.6	SPEED (RPM)		1726
29	MOTOR (Munsell No)		0.6PB 4.8/10.6	INSULATION CLASS		F
30	LUBRICATION FLUID		GEAR BOX (GEAR OIL)	PROTECTION DEGREE		IP54
31	WEIGHTS (kg)		21	HUB SIZE		Ø22
32	ACCESSORIES			SPARE PARTS
33	□ RELIEF VALVE □ BACK PRESS VALVE			□ PLUNGER □ BALL SEAT
34	□ ACCUMULATOR(AIR CHAMBER)			□ CHECK BALL □ BALL GUIDE
35	□ PRESSURE GAUGE			□ GLAND PACKING □ VALVE GASKET
36	REMARKS:
37

CHEON-SEI IND.CO.,LTD.